0x05F4 Statistics Update Timer

Use this TLV in the Generic Card Configure message to set how often system statistics are updated.

Byte | Description
0, 1 | Tag: 0x05F4 - Statistics Update Timer
2, 3 | Length: 0x0002
4, 5 | Value[0, 1] - Timer Value Minimum: 1 (0x0001) Maximum: 168 (0x00A8) Default: 24 (0x0018)

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.