L3P TUP Configuration Bytes

Byte | Description | Value
--- | --- | ---
0x01 | Answer Type | 0x00=ANC (default) 0x01=ANN 0x02=ANU
0x02 | CCL Reception Processing Options | 0x00=Auto-reply w/ CBK (default) 0x01=Send PPL Event (CCL) to host
0x03 | Outgoing Call Release Option | 0x00=CLF (default) 0x01=CCL
0x04 | Host-initiated OOS | 0x00=BLK/UBL (default) 0x01=RSC
0x05 | CBK Reception Processing Options | 0x00=Auto-reply with CLF (default) 0x01=PPL Event (CBK) to host
0x06 | RFS Format | 0x00=TUP Fields (default) 0x01=BCD Encoded Digits
0x07 | Send ACM PPL Event to host | 0x00=Do Not Send (default) 0x01=Send
0x08 | Send Answer PPL Event to host | 0x00=Do Not Send (default) 0x01=Send
0x09 | Outgoing Congestion Control | 0x00 - Disable 0x01 - Enable (default)
0x0A | Enable/Disable PPL Event Indication sending to host. 1=Send PPL Event Indication to host. 0=Do not send PPL Event Indication to host. If this byte is set to "1", all the block/unblock acknowledgments and reset complete indications (RLG) will be sent to the host. | 0x00 NOTE: Config Byte 0x0A is used only for China TUP customized PPLs.
0x0B | Send Auto ACM 0=Wait for Host initiated ACM 1=Generate ACM using default parameters | 0x00
0x0C-0x0E | Unused |
0x0F | Field ID of Called Party Address | 0x03
0x10 | Field ID of Calling Line ID | 0x08
0x11 | Address Indicator for Calling Line ID | 00x0
0x12-0x13 | Unused |
Address Complete Message (ACM)
0x14 | Number of Fields | 0x01
0x15 | ACM Message Indication Fields | 0x0C
0x16 | Field Length | 0x01
0x17 | Field Data | 0x00
0x18-0x1D | Unused |
General Request Message (GRQ)
0x1E | Number of Fields | 0x01
0x1F | GRQ Message Indication Fields | 0x0D
0x20 | Field Length | 0x01
0x21 | Field Data | 0x00
0x22-0x27 | Unused |
Automatic Congestion Control Message (ACC)
0x28 | Number of Fields | 0x01
0x29 | ACC Message Indication Fields | 0x13
0x2A | Field Length | 0x01
0x2B | When set will cause a REL to be sent to the network prior to transitioning into the In Service Protocol. | 0x00 (default) 0x01 - Send REL to Network
0x2C-0x31 | Unused |
Extended Unsuccessful Backward Setup Information Message (EUM)
0x32 | Number of Fields | 0x02
0x33 | EUM Octet Indication Fields | 0x14
0x34 | Field Length | 0x01
0x35 | Field Data | 0x01
0x36 | SPC | 0x15
0x37 | Field Length | 0x02
0x38 | Field Data | 0x00
0x39 | Field Data | 0x00
0x3A-0x3B | Unused |
Initial Address Message (IAM)
0x3C | Number of Fields | 0x02
0x3D | Calling Party Category | 0x01
0x3E | Field Length | 0x01
0x3F | Field Data | 0x0A
0x40 | Field ID | 0x02 - Call Setup Message Indicators
0x41 | Field Length | 0x02
0x42 | Field Data | 0x00
0x43 | Field Data | 0x00
0x44-0x4F | Unused |
Initial Address Message with Initial Information (IAI)
0x50 | Number of Fields | 0x02
0x51 | Calling Party Category | 0x01
0x52 | Field Length | 0x01
0x53 | Field Data | 0x0A
0x54 | Field ID | 0x02 - Call Setup Message Indicators
0x55 | Field Length | 0x02
0x56 | Field Data | 0x00
0x57 | Field Data | 0x00

See Programmable Protocol Language.
A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
Out of Service
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.
See Request For Service.
Telephone User Part