0x4E22 Message Processing Supported

The following table defines the format of the Message Configuration Supported TLV:

Used in:
SS7 ISUP Message Format Configure message

Byte | Description
0, 1 | Tag 0x4E22
2, 3 | Length 0x0001
4 | Value[0] 0x00 Not Supported 0x01 Supported (Default)

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
See Signaling System Number Seven.
See Integrated Services Digital Network User Part.