0x01C3 Maximum Jitter Buffer Delay (IPN-3 Card)

The data in this TLV block are in millisecond units. The range of legitimate values is 0-200 ms.

Used in:
0x1E and 0x001E Generic PPL ICBs in:
Resource Attribute Query message
Resource Attribute Configure message

Byte | Description
0, 1 | Tag 0x01C3 Maximum Jitter Buffer Delay
2, 3 | Length 0x0004
4 | Value[0] 0x00
5 | Value[1] 0x00
6, 7 | Value[2, 3] 0x0000-0x00C8 0x0096 (Default)

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
See Programmable Protocol Language.