0x01C4 Adaptation Rate

Use this TLV to configure the Adaption Rate on a VDAC-ONE card.

The data in this TLV block are in millisecond units. The range of legitimate values is 0-12 milliseconds.

Used in:
0x1E and 0x001E Generic PPL ICBs in:
Resource Attribute Query message
Resource Attribute Configure message

Byte | Description
0, 1 | Tag 0x01C4 Adaptation Rate
2, 3 | Length 0x0001
4 | Value[0] 0x00-0x0C (0x07 Default)

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
See Programmable Protocol Language.