0x0005 IP Signaling Series 3 Card Slot Number

Used in:
IP Signaling Series 3 Card Configure message (0x0100)
IP Signaling Series 3 Card Query message (0x0101)

Byte | Description
0, 1 | Tag 0x0005
2, 3 | Length 0x0002
4 | Value[0] IP Signaling Series 3 Card Slot Number, MSB 0x00
5 | Value[1] IP Signaling Series 3 Card Slot Number, LSB 0x00-0x0F

Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
Most Significant Bit
Least Significant Bit