You are here: SwitchKit® Development Environment - Installation and Maintenance Guide > 5 Building a Configuration File > API Messages Used for Configuration

API Messages Used for Configuration

This section outlines the messages available for various types of configuration related to the following:

• Common SwitchKit API

• Common EXS API

• Common Call Control

• Channel Associated Signaling

• Common Channel Signaling

• Digital Signal Processor

• System-related

• PPL

Finding the Messages

Information about each of the messages in this section is in the SwitchKit API Reference. The messages in the sub-categories that follow have links to them in the API reference. In the chapters that follow this one, you find API messages related to device connectivity, line card switchovers and server status.

Common SwitchKit

AddLLCCard
AddLLCNode
AdjustMessageTimeout
AllInService
AllOutOfService
AssociateChanGroup
ClearAllChanGroups
ClearChanGroup
ConfigChanGroup
HexTool
RecordedAnnouncement

Common EXS API

AnswerSuperviseConfig
AssignSpan
BusyOutFlagConfig
DistantReleaseConfig
FlashTimingConfig
GenericCardConfigure
GenericCardQuery
InpulsingParametersConfig
InseizeInstrListConfig
IPAddressConfig
LocalReleaseConfig
LoopTimingConfig
MultiHostConfig
OuseizeInstrListConfig
ProductLicenseDownload
ResetConfig
ResourceAttributeConfig
ServiceStateConfig
Standby Line Card Config
SynchPriorityConfig
SystemConfig
TimeSet

Common Call Control

CrossConnectChannel
CrossConnectSpan
CrossDisconnectChannel
CrossDisconnectSpan

Channel Associated Signaling

DS3GenericMessage
E1SpanConfig
T1SpanConfig
LoopBackConfig
PCMEncodingConfig
ReceiveSignalingConfig
Span Filter Config
StartDialConfig
TransmitSignalingConfig
TrunkTypeConfig

Common Channel Signaling

CCSRedundancyConfig
SS7 Configuration Messages
SS7CICConfig
SS7CLLIConfig
SS7ISUPMessageFormatConfig
SS7SCCPTCAPConfig
SS7SignalingLinkConfig
SS7SignalingLinkSetConfig
SS7SignalingRouteConfig
SS7SignalingStackConfig
SS7TUPMessageFormatConfig
VitualSlotConfig
VirtualSpanControl
ISDN & V5 Configuration Messages
BChannelConfig
DChannelAssign
DChannelDeAssign
DChannelFacilityListConfig
ISDNInterfaceConfig
ISDNTerminalConfig
V5Config

Digital Signal Processor

ConferenceCreate
ConferenceDeleted
ConferenceDeleteRequest
ConnectToConference
ConnectOneWayToConference
ConnectOneWayForced
CPAClassConfig
CPAPatternConfig
DSPCacheModify
DSPSIMMConfig
PlayFileModify
PlayFileStart
PlayFileStop
RecAnnConnect
RecAnnDelete
RecAnnDisconnect
RecAnnDownload
RecAnnDownloadInit
RecAnnFSConvert
RecAnnFSDefrag
RecAnnSingleDelete
RecordFileModify
RecordFileStart
RecordFileStop
RecAnnConnect
Resource Create
ResourceDelete
Resource Modify
TransmitCadencePatternConfig
TransmitToneConfig

System-Related

AssignEXSHostSlave
NodeConfig
RingConfig

PPL

PPLAssign
PPLAuditConfig
PPLConfig
PPLDelete
PPLEventRequest
PPLTimerConfig
PPLTransmitSignalConfig

Setting up, monitoring, and tearing down calls.
CAS. Signaling in which the signals necessary to switch a given circuit are transmitted via the circuit itself or via a signaling channel permanently associated with it.
CCS. Network architecture using SS7 protocol for the exchange of information between telecommunications nodes and networks on an out-of-band basis.
See Programmable Protocol Language.
Range of channels provided by T1 or E1 transmission service. A physical span is a group of channels taking up a single physical wire. A logical span is a group of channels taking up less than a single logical wire, or carried over more than one physical wire.
See Signaling System Number Seven.
See Integrated Services Digital Network.