0x09 Ethernet Link Redundancy

Use this TLV to enable Ethernet Link Redundancy. If you enable Ethernet Link Redundancy, the lower Ethernet Port is automatically activated. Note that Ethernet Link Redundancy is not supported on the SS7 Series 3 card.

Used in:
IP Address Configure message
IP Address Query message

Byte | Description
0 | Tag 0x09 Ethernet Link Redundancy
1 | Length 0x04
2-5 | Value[0-3] 0x00000000 Disable 0x00000001 Enable

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
The protocol used in most local area PC networks. Typically, most Ethernet networks support data transmission speeds up to 10 Mbps, but 100 Mbps is also possible.
The point in the Excel platform where a DS0 connects to a network. Also known as a "socket."
See Signaling System Number Seven.
Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
A 32-bit address, used in IP routing, which includes a Network address identifier assigned by a central authority and a Host ID (an end station identifier assigned by a LAN administrator).