0x294E SIP Remote IP Address

This TLV reports the IP Address of the remote socket.

Used in:
0x0033 NPDI Universal ICB in:
Request for Service message

Byte | Description
0, 1 | Tag 0x294E
2, 3 | Length 0x0004
4-n | Value[0-n] MSB of the IP Address LSB of the IP Address

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
Network Protocol Data Intelligence. Also called “Interworking,” it is a software product that operates within Excel’s Call Control (Layer 4) and Services (Layer 5) call processing layers. NPDI is meant to enhance Excel’s call processing product offering by allowing call processing layers (specifically Layers 4 and 5) to perform advanced analysis, generation, and conversion of Network Signaling (NS) Layer 3 information.
See Information Control Block.
Most Significant Bit
A 32-bit address, used in IP routing, which includes a Network address identifier assigned by a central authority and a Host ID (an end station identifier assigned by a LAN administrator).
Least Significant Bit