VoIP

Comp. ID | Comp. Name | PPL Assign | PPL Audit Config. | PPL Audit Query | PPL Config. | PPL Data Query | PPL Event Request/ Indication | PPL Timer Config.
--- | --- | --- | --- | --- | --- | --- | --- | ---
0x009C | VDAC-ONE VoIP | N/A | Channel 0x0D | N/A
0x009F | IP Network Interface Series 2 VoIP | Channel 0x0D | N/A

See Programmable Protocol Language.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.
Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).
Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.