You are here: CSP Developer’s Guide: Overview > 11 Call Routing > Host Notification of Route Derivation

Host Notification of Route Derivation

You can configure the router to send a Request For Service message to a specific host port after a route has been derived.

Figure 11-10 Host Port Routing of Request for Service

Configuration

To enable this feature, insert the following TLVs into the PPL Config Bytes of the CH component:

• Special Instructions TLV (0x001D)

• Instruction # 0x01 (Allocate Entity)

• Send Route Control to Router TLV (0x004D)

See the API Reference for information on TLV formats.

RFS. A Status Message indicating that some entity is requesting service from the Excel platform.
A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
The point in the Excel platform where a DS0 connects to a network. Also known as a "socket."
See Programmable Protocol Language.
Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.