MTP3 HMRT PPL Event Requests (AIB: Stack/Link 0x08)

Event ID | Event
--- | ---
0x0001 | Start or restart interval reporting. If restarting the measurement interval, this event will result in reports for the current measurement interval before restarting.
0x0002 | Stop interval reporting. Immediately stop interval reporting.
0x0A | TRANSFER REQ Used to send MSU data Parameter ID - 0x0424, 0x0425, 0x0426

In PPL, a condition that, when met, drives a state machine (PPL Component) from one state to another, by invoking an associated Primitive. In PPL files, an Event is marked by an arrow and text.