0x0274 Use No Local Media

Use this TLV to specify the way to handle a situation where there is no VDAC-ONE or IP Network Interface Series 2 card.

Used in:
VoIP Protocol Configure message
VoIP Protocol Query message

Byte | Description
0, 1 | Tag 0x0274
2, 3 | Length 0x0001
4 | Value[0] Media Handling 0x00 Not in the media path - no VDAC-ONE or IP Network Interface Series 2 cards available 0x01 Terminate media locally - VDAC-ONE or IP Network Interface Series 2 cards (Default)

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).