You are here: SwitchKit® Development Environment - TCAP Interface User’s Guide > 6 SKTAL Parameter Classes > Class TCAP_Result : public TCAP_Component

Class TCAP_Result : public TCAP_Component

Purpose

The purpose of the TCAP_Result component is to define the basic interface to remote operation results. This class is used to reply to successful invoke operations.

Summary of Methods

The TCAP_Result component includes the following methods:

// Operation

//If defined(CCITT)

void SetOperation(const SKTAL_LONG code);

void GetOperation(SKTAL_LONG& code) const;

// parameter

void SetParameter(const SKTAL_OCTET* buf, const int len);

void GetParameter(SKTAL_OCTET* buf, int& len) const;

void SetParameter(const SKTAL_ByteArray& buf);

void GetParameter(SKTAL_ByteArray& buf) const;

SetOperation()

Description

This method sets the operation field of a result component. The SetOperation method is relevant only to ITU TCAP.

Syntax

void Set Operation(const SKTAL_LONG code);

Input Parameters

code: The operation code.

Input/Output Parameters and Output Parameters

None

Return Value

None

GetOperation()

Description

This method gets the operation field of an invoke component. The GetOperation method is relevant only to ITU TCAP.

Syntax

void GetOperation(SKTAL_LONG& code) const;

Input Parameters and Input/Output Parameters

None

Output Parameters

code - The operation code

Return Value

None

SetParameter()

Description

Copies a user-defined parameter into the invoke component.

Syntax

See class TCAP_Invoke

void SetParameter(const SKTAL_OCTET* buf, const int len);

void SetParameter(const SKTAL_ByteArray& buf);

Input Parameters

buf - A buffer containing the parameter to copy into this component

len - The length of the parameter in the buffer.

Input/Output Parameters & Output Parameters

None

Return Value

None

GetParameter()

Description

Copies a user-defined parameter from the invoke component to a user supplied buffer.

Syntax

void GetParameter(SKTAL_OCTET* buf, int& len) const;

void GetParameter(SKTAL_ByteArray& buf) const;

Input Parameters

buf: a buffer containing the parameter to copy into this component

Input/Output Parameters

None

Output Parameters

len - The length of the parameter in the buffer.

Return Value

None

See Transaction Capability Application Part.
Comité Consultatif Internationale de Telephonique et Telegraphique (now ITU)
A sequence of eight bits.
International Telecommunications Union (UN)