0x0014 Message Header Information

Used in:
PPL Event Indication message

Byte | Description
0, 1 | Tag 0x0014
2, 3 | Length 0x0004
4, 5 | Value[0-1] Contains the message type 0x00E8 - Route Control or 0x002C - Outseize Control
5,6 | Value[2-3] Contains the two-byte sequence number of the Route Control /Outseize Control message sent by the host. The valid values ranges from 0x0000-0xFFFF.

See Programmable Protocol Language.
Outgoing call setup during real-time call processing on a specific channel.