0x0262 Use SIP Local Port

Use this TLV to specify the local SIP port number. The default port number is 0x13C4 (5060).

Used in:
VoIP Protocol Configure message

Byte | Description
0, 1 | Tag 0x0262
2, 3 | Length 0x0002
4, 5 | Value[0,1] Port Number

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Session-Initiation Protocol. A signaling protocol used for establishing sessions in an IP network. A session could be a simple, two-way telephone call, or it could be a collaborative multi-media conference session.
Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).
The point in the Excel platform where a DS0 connects to a network. Also known as a "socket."