0x01 Scan For Wink N

Used in:
Route Control message
Outseize Control message

ICB Type | 0x01 (Action)
ICB ID | 0x01 Scan for Wink N
Data Length | 0x01
Data[0] | Wink Number (0x01–0x08)

Outgoing call setup during real-time call processing on a specific channel.
See Information Control Block.
Momentary interruption in a single frequency tone indicating the distant switch is ready to receive the digits just dialed.