You are here: SwitchKit® Development Environment - CSA User’s Guide > 4 Configuring Signaling Cards > Dual Port Usage for SS7 Series 3 Card

Dual Port Usage for SS7 Series 3 Card

Configuring Port A, Port B

This procedure describes how to configure two ports for your SS7 card. For more information see the Developer’s Guide: CCS, Dual Ethernet Port for SS7 Series 3 Card (2-105).

1 Open a node view.

2 Right-click the SS7 card in its slot.

3 Select IP Address Configure from the menu.

4 Enter the IP Address, Subnet Mask and Gateway for Port A.

5 Enter the IP Address, Subnet Mask and Gateway for Port B.

6 Click OK.

The point in the Excel platform where a DS0 connects to a network. Also known as a "socket."
See Signaling System Number Seven.
See Common Channel Signaling.
The protocol used in most local area PC networks. Typically, most Ethernet networks support data transmission speeds up to 10 Mbps, but 100 Mbps is also possible.
Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
A 32-bit address, used in IP routing, which includes a Network address identifier assigned by a central authority and a Host ID (an end station identifier assigned by a LAN administrator).
The bits of an Internet Protocol (IP) address used for a subnetwork.
A device that translates calls between an IP network and another network, typically the PSTN.