You are here: SwitchKit® Development Environment - TCAP Interface User’s Guide > 5 SwitchKit TCAP Abstraction Layer > sktal_recvTCAPDialog()

sktal_recvTCAPDialog()

Description

This method receives TCAP dialogue information from a SKTAL_EVENT.

Syntax

int sktal_recvTCAPDialog(int instanceId, SKTAL_EVENT *ev,

unsigned *dialogueId, SKTAL_DLG *dlg);

Input Parameters

instanceId: instance for registered node/stack/snn combination.

ev: event containing dialogue information.

The SKTAL_EVENT is defined in Appendix C.

Input/Output Parameters

None

Output Parameters

Argument | Description
--- | ---
dialogueId | TCAP dialogue ID
dlg | Pointer to the structure containing TCAP dialogue information

For definition see Appendix D, SKTAL_DLG and SKTAL_CPT Structure Definitions.

Return Value

SKTAL_SUCCESS: If method is successful.

SKTAL return code as defined in Appendix C, SKTAL Return Codes.

See Transaction Capability Application Part.
In PPL, a condition that, when met, drives a state machine (PPL Component) from one state to another, by invoking an associated Primitive. In PPL files, an Event is marked by an arrow and text.