0x064B Receive Bad Line

Use this TLV in the Generic Card Configure (0x0122) and Resource Connect (0x0127) messages to set the action to take for the placement of bad lines in an image.

Byte | Description
0, 1 | Tag: 0x064B Receive Bad Line
2, 3 | Length: 0x0002
4, 5 | Value[0,1]: Action to take for placement of bad lines in the image 0x0000 Do Nothing 0x0001 Repeat Last Good Line (Default) 0x0002 Blank Line with Tic Marks on Each Side 0x0003 Blank Line

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.