You are here: CSP Hardware Product Descriptions > 6 Resource Cards > Dialogic® Digital Signal Processing Series 2 Card - See Model Numbers

Dialogic® Digital Signal Processing Series 2 Card - See Model Numbers

Description

You can order the Dialogic® Digital Signal Processing Series 2 Card with either one or two DSP modules. The one-module card is the CSP-DSP 1310. The two-module card is the CSP-DSP 1320. Each module consists of four DSP chips, for a total of either four or eight DSP chips per card. Each DSP chip has access to 512 timeslots of PCM. The 512 timeslots are arranged in two streams of 256 timeslots each. Each DSP is controlled through a host port interface mapped into the main board’s memory space.

The DSP Series 2 card main board has 128 Mbyte of external synchronous SDRAM and 2 MBytes of Flash memory. The processor is a HIP4 8260 running at 83 Mhz.

Ethernet Switch

The main board has an internal Ethernet switch, and brings out three external 100 Base-T Ethernet ports to the I/O. These three ports can be used for redundancy.

Function

The DSP Series 2 card can perform a single function or a combination of the following functions:

• Tone generation

• Tone detection

• Conferencing

• File Playback/Record

• Signal energy detection

Placement

The DSP Series 2 card resides in the front slot of the following CSP chassis:

CSP 2040

Two fully-loaded DSP-2 cards can operate in an CSP 2040 Chassis.

CSP 2090 and CSP 2110

Five fully-loaded DSP-2 cards can operate in the CSP 2090 and CSP 2110 chassis.

Configuration Information

The part number, serial number, model number, and revision number are located on the back of the card.

Specifications

The DSP Series 2 card is designed to the following electrical, physical, and environmental specifications.

Electrical | Specification
--- | ---
Supply Voltage, Vcc | 5.00V
Supply Current, Vcc @ 5.0V | 5.5A (typical)

Physical | Specification
--- | ---
Height | 9.3 inches (236.2 mm)
Depth | 12.5 inches (317.5 mm)
Width | .775 inches (19.7 mm)

Environmental | Specification
--- | ---
Temperature - Storage | -40~C to 70~C (-40~F to 158~F)
Temperature - Operation | 0~C to 50~C (32~F to 122~F)
Temperature Shock - Storage | -40~C to 70~C to -40~C (-40~F to 158~F to -40~F) at 5~C/min.
Temperature Shock - Operation | 0~C to 50~C (32~F to 122~F) at 10~C/min.
Humidity - Operating | 5% to 85%
Altitude | Up to 4000 meters (13,123 ft.)

Power Requirements

Configuration | Min. Current at 5V | Max Current at 5V | Minimum Power | Maximum Power
--- | --- | --- | --- | ---
DSP Series 2 with one Module | 4.2 | 4.4 | 21.0 | 22.0
DSP Series 2 with two Modules | 5.2 | 5.5 | 26.0 | 27.5

DSP Series 2 Card Models

The available DSP Series 2 card models are listed below.

Product | Model No. | RoHS Model No.
--- | --- | ---
DSP Series 2 with (1) Module | CSP-DSP 1310 | CSP-DSP 1310R
DSP Series 2 with (2) Modules | CSP-DSP 1320 | CSP-DSP 1320R

Related Products

The products related to the DSP Series 2 card are listed below.

Product | Model No. | RoHS Model No.
--- | --- | ---
Multi-Function Media I/O | CSP-BIO-1000 | CSP-BIO-1000R

Front and Top Views

The front and side views show the LEDs, push button switches, Monitor connector, DIP switches, and jumpers.

Controls and Indicators

The table below describes the LEDs and push button switches as shown in the front view of the DSP Series 2 card.

Status Indicators

LED indicators reference standard CPU run/halt/reset statuses.

LED | Color/Status | Description
--- | --- | ---
Diag | Off | This LED is OFF except during a card reset, when this card flashes red briefly.
Status | Red | The LED is red briefly during card reset.
Green | The card is connected to the system buses.
Off | The card is resetting.
Halt | Red | The CPU has halted. This LED is red briefly during card reset.
Green | The CPU is running.
Power | Red | The LED is red upon insertion
Green | The card is In Service.
Off | The card is Out Of Service.

Jumpers

The table below indicates the jumper settings.

Jumper | Setting | Description
--- | --- | ---
J1009 | Installed (default) | Factory use only
J1010 | Installed (default) | Factory use only
J1011 | Installed (default) | Factory use only
J1013 | Not Installed (default) | Factory use only
J1014 | Not Installed (default) | Factory use only
J1015 | Not Installed (default) | Factory use only
GJ1000 | Not Installed (default) | Factory use only

DIP Switch S1 on Main Board

The table below describes the DIP switch S1 settings. The shading (asterisk* for html documents) indicates factory-installed settings.

Position | Setting | Function
--- | --- | ---
1 | ON* | Disables Debug 1 Mode
OFF | Enables Debug 1 Mode ( printing)
2 | ON* | Reserved, normally should be ON
OFF | Reserved
3 | ON* | Disables Debug 2 Mode
OFF | Enables Debug 2 Mode
4 | ON* | Ethernet Link, Auto-Negotiate Mode (Default)
OFF** | Ethernet Link, Force 100 Mbps/Full Duplex Mode
5 | ON* | Reserved, normally should be ON
OFF | Reserved
6 | ON* | HDLC Communications (Default)
OFF | Ethernet Communications***
7 | ON* | Reserved, normally should be ON
OFF | Reserved
8 | ON* | Reserved, normally should be ON
OFF | Reserved

** Enables Ethernet Link, Force 100 Mbps/Full Duplex feature.

*** Enables Ethernet communication between the DSP Series 2 card and the CSP Matrix Series 3 Card.

Digital Signal Processor
See Pulse Code Modulation.
Quick depress and release of the phone plunger of a handset to signal the PBX or Centrex of instructions to follow (e.g., Call Transfer).
The protocol used in most local area PC networks. Typically, most Ethernet networks support data transmission speeds up to 10 Mbps, but 100 Mbps is also possible.