0x060D Automatic Gain Control Input Level

Use this TLV in the Resource Create (0x0124) and Generic Card Configure messages (0x0122) to set the target input level in conferences.

Byte | Description
0, 1 | Tag: 0x060D Automatic Gain Control Input Level
2, 3 | Length: 0x0002
4, 5 | Value[0, 1]: Input Level (1 dBm steps) Min: -54 (0xFFCA) Max: -3 (0xFFFD) Default: -22 (0xFFEA)

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.