0x0668 Transmit dbm Level

Used in: Generic Card Configure (0x0122), Generic Card Query (0x0123), Resource Connect (0x0127), and Resource Query (0x012C) messages.

Byte | Description
0, 1 | Tag 0x0668 Transmit dbm Level
2, 3 | Length 0x0002
4, 5 | Value[0,1] dbm level for G.711 transmission in tenths of dbm. -400 to 0dbm. Min -400 (0xFE70) Max 0 Default -135 (0xFF79)

(Not supported in the current release.)