You are here: CSP Developer’s Guide: Overview > 9 Configuring the DSP-ONE Card > Recorded Announcement Call Flows

Recorded Announcement Call Flows

The diagram below shows a simple example of how the VRA features play out a greeting.

Trunk Type:E&M Wink Start

Inseize Control Instructions:

1. Generate Inseize Acknowledgment (Wink 1)

2. Report Incoming Call

3. Wait for Host Control

Description

1. Receive incoming call

2. Play out greeting

3. Receive Call Processing Event of "Recorded Announcement Complete"

4. Send Release Channel 0x0008 message

Momentary interruption in a single frequency tone indicating the distant switch is ready to receive the digits just dialed.
A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.