L3P Protection Protocol PPL Timers (0x008E)

When specifying new timer values, remember that all PPL Timers are specified in 10 ms increments. For example, a PPL timer for 4 seconds is specified as 4000 (decimal, 400 x 10 ms = 4 seconds), which is the hexadecimal value of (0x190).

Timer ID | Description | Value (default)
--- | --- | ---
0x01 | Waiting for Switchover Acknowledge | 1.5 seconds
0x02 | Waiting for Switchover Acknowledge | 1.5 seconds
0x03 | Waiting for Switchover Com | 1.5 seconds
0x04 | Waiting for Reset SN Acknowledge | 20 seconds
0x05 | Will always expire | 10 seconds

See Programmable Protocol Language.