0x01E0 ARP Cache Report Information

This TLV is sent in the ARP Cache Report message to indicate the number of messages required for the report and the number of the current message.

Byte | Description
0 | Tag 0x01E0
1 | Length 0x0002
2 | Value[0] Number of ARP Cache Report messages
3 | Value[1] Current Message Number

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.