0x0080 IP Signaling Series 3 Card Status

Used in:
Matrix Status Report message (0x00E5)

Byte | Description
0, 1 | Tag 0x0080
2, 3 | Length 0x0004
4, 5 | Value[0, 1 ] DSM FM State Values 0x00FF FSM uninitialized 0x0001 FSM initialized 0x0002 FSM waiting for Socket Accessible Indication 0x0003 FSM waiting for Socket Inaccessible Indication 0x0004 FSM waiting for Status Indication from the IP Signaling Series 3 Card 0x0005 FSM waiting for Span Status query 0x0006 FSM waiting for Span Status change indication 0x0007 FSM waiting for Channel Status Indication from the IP Signaling Series 3 Card 0x0008 FSM waiting for Channel Status Complete from the IP Signaling Series 3 Card 0x0009 FSM active 0x000A FSM inactive
6, 7 | Value[2, 3] IP Signaling Series 3 Card Status Information 0x0000 IP Signaling Series 3 Card status information (received device server status indication) 0x0001 Type did not authenticate 0x0002 Configuration Tag did not authenticate 0x0003 Compatibility Tag did not authenticate 0x0004 IP Signaling Series 3 card socket inaccessible 0x0005 IP Signaling Series 3 card socket accessible (at least one active socket to IP Signaling Series 3 card) 0x0006 Socket open failure 0x0007 Socket close failure 0x0008 IP Signaling Series 3 card active IP Signaling Series 3 available to process calls) 0x0009 IP Signaling Series 3 card link down (socket connection is open, but the IP Signaling Series 3 card is not responding to poll requests)

The condition of a component at a given instant. The current "context" of a PPL object, such as Idle, Seizing, Answered. In PPL files, a State is represented by a circle.
Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
Range of channels provided by T1 or E1 transmission service. A physical span is a group of channels taking up a single physical wire. A logical span is a group of channels taking up less than a single logical wire, or carried over more than one physical wire.