0x0009 Terminating Channel

Use this TLV to specify a destination channel or a node. This TLV is used for the Terminating Channel routing method. The span/channel or node are specified in the TLV in an Address Information Block (AIB).
Used in:
0x001E or 0x1E Generic PPL ICB in Route Control message

Byte | Description
0, 1 | Tag 0x0009 Terminating Channel or Node
2, 3 | Length 0x0005
4 | Value[0] AIB Type: 0x0D
5 | Value[1] AIB Length (0x03)
6 | Value[2] Logical Span (MSB)
7 | Value[3] Logical Span (LSB)
8 | Value[4] Channel

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
AIB. A standardized block that allows address data to be inserted in a standard way into API messages.
See Address Information Block.
See Programmable Protocol Language.
See Information Control Block.
Range of channels provided by T1 or E1 transmission service. A physical span is a group of channels taking up a single physical wire. A logical span is a group of channels taking up less than a single logical wire, or carried over more than one physical wire.
Most Significant Bit
Least Significant Bit