L3P PSTN PPL Timers

When specifying new timer values, remember that all PPL Timers are specified in 10 ms increments. For example, a PPL timer for 4 seconds is specified as 4000 (decimal, 400 x 10 ms = 4 seconds), which is the hexadecimal value of (0x190).

Timer ID | Description | Value (default)
--- | --- | ---
0x01 | Layer 3P BCC Response Wait | 8 seconds
0x02 | Signal (On-hook/Normal Polarity)/Disconnect Complete Wait | 4 seconds
0x03 | Layer 3 Digit Wait Timer | 4 seconds
0x04 | Layer 4 Clear Wait Timer | 4 seconds
0x05 | Layer 3 Establish Acknowledge Wait | 4 seconds

See Programmable Protocol Language.
Protocol layer of the CSP.
Call processing layer of the CSP.