SCCP SUSI Configuration Bytes

Byte | Description | Value
--- | --- | ---
0x01 | PPL Event Indication format | 0x00=Use RAW CGPA and CDPA format in PPL Event Indication. (default) 0x01=Use CGPA and CDPA Elements format in PPL Event Indication
0x03 | Maximum length of data to the host in PPL Event Indications | 0xF0 (default)
0x12 | ICB format for indications | 0x00 - Data ICB (default) 0x01 - Extended ICB format
0x14-0x17 | Used to store the maximum allowable to the host for ICB length in the SCCP PPL Event Indication. | 0xF0 (default)

See Programmable Protocol Language.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.
See Information Control Block.