MTP2 PPL Timers for other components (ANSI)

PPL Component | Timer ID | Timer | Default Value (10 ms)
--- | --- | --- | ---
CC | 0x01 | T1.111/T5 | 10
IAC (0x0022) | 0x01 | T1.111/T2 | 1150
0x02 | T1.111/T3 | 1150
0x03 | T1.111/T4N | 230
0x04 | T1.111/T4E | 60
LSC (0x0023) | 0x01 | T1.111/T1 | 1300

See Programmable Protocol Language.
Digital communications link - voice, data, and video at a 1.544 Mbps rate (24 64 Kbps channels)
ANSI Publication on Functional Description of MTP
Digital communications link - 44.378 Mbps rate