0x65 TCAP Primitive

Used in:
PPL Event Indication message
PPL Event Request message

ICB Type | 0x02 (Data)
ICB ID | 0x65
Data Length | 0x0nn
Data[0-3] | TCAP Dialogue ID
Data[4-5] | TCAP TC-Primitive ID
Data[6+] | TCAP TC-Parameter TLVs
: | :

See Programmable Protocol Language.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.
See Information Control Block.
See Transaction Capability Application Part.