0x01DC VoIP Module

Use this TLV to indicate a VoIP module.

Used in:
0x00FB ARP Cache Report message

Byte | Description
0, 1 | Tag 0x01DC VoIP Module
2, 3 | Length 0x0001
4 | Value[0] Module Number

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).