You are here: CSP Developer’s Guide: Overview > 7 Configuring and Using Resources on the DSP Series 2 Cards > Configuring Conferencing Options

Configuring Conferencing Options

Feature Description

See Conferencing Options.

Conferencing Options TLVs

TLV (Optional unless Noted) | Notes/Values * = default
--- | ---
0x05E5 Barge In | By default, Barge-In is enabled for conferencing. Include this TLV to disable it. 0x0000 - Disabled 0x0001 - Enabled *
0x0604 DTMF Clamping/Filtering Enable | Use this TLV to enable DTMF filtering. 0x0000 - Disabled* 0x0001 - Enabled
0x0605 EXS Conferencing Encoding Type | Use this TLV to specify the encoding type for a conference over the EXNET® ring. 0x0000 - u-law 0x0001 - A-law 0x0002 - Mixed *

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.