You are here: SwitchKit® Development Environment - CSA User’s Guide > 7 System Provisioning and Monitoring > Disable Ethernet Redundancy

Disable Ethernet Redundancy

Right-click the DSP-S2 card and select the menu option, Disable Ethernet Redundancy.

Click Yes in the next dialog box.

The next dialog box confirms that Ethernet Redundancy is disabled.

Digital Signal Processor
The protocol used in most local area PC networks. Typically, most Ethernet networks support data transmission speeds up to 10 Mbps, but 100 Mbps is also possible.