0x295A SIP RPID Privacy

Used in:
Request for Service with Data (0x002D)
PPL Event Indication (0x0043)
PPL Event Request (0x0044)
Route Control (0x00E8)
Outseize Control (0x002C)

Byte | Description
0, 1 | Tag 0x295A
2, 3 | Length Variable (Maximum of 250 bytes when used in Outseize or Route Control or subsequent PPL Event Request messages)
4-n | Value Contains the value of the RPID Privacy header as a null terminated ASCII string.

See Programmable Protocol Language.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.
Outgoing call setup during real-time call processing on a specific channel.
American Standard Code for Information Interchange