You are here: CSP API Reference > 1 EXS & SwitchKit API Messages > Card Population Query 0x0007

Card Population Query 0x0007

SwitchKit Name

CardPopulationQuery

Type

EXS API and SwitchKit API message

Description

Card Population Query 0x0007

Use this message to query the cards installed in the system. The response indicates the Card Type installed in each slot (or virtual slots) in the system.

Related Information

Chassis Slot Numbering

Card Types

Sent by

Host

SwitchKit Code

C Structure

typedef struct {

} XL_CardPopulationQuery;

C Structure Response

typedef struct {

unsigned short Status;

UBYTE Info[96];

} XL_CardPopulationQueryAck;

C++ Class

class XLC_CardPopulationQuery : public XLC_OutboundMessage {

public:

};

C++ Class Response

class XLC_CardPopulationQueryAck : public XLC_AcknowledgeMessage {

public:

unsigned short getStatus() const;

void setStatus(unsigned short x);

const UBYTE *getInfo() const;

UBYTE *getInfo();

void setInfo(UBYTE *x);

};

Overview of message

The following table provides an overview of this message. The table following it provides the detail for each byte.

MESSAGE (White) | RESPONSE (Gray)
Byte | Field Description | Byte | Field Description
0 | Frame (0xFE) | 0 | Frame (0xFE)
1, 2 | Length (0x0005) | 1, 2 | Length (0x0067)
3, 4 | Message Type (0x0007) | 3, 4 | Message Type (0x0007)
5 | Reserved (0x00) | 5 | Reserved (0x00)
6 | Sequence Number | 6 | Same Sequence Number
7 | Logical Node ID | 7 | Logical Node ID
8 | Checksum | 8, 9 | Status (MSB, LSB)
| 10 | Slot 0* Card Type
11 | Slot 1* Card Type
73 | Card Type
74-105 | Slot 63 Card Type
106 | Checksum

EXS API Hex Format - Detailed

MESSAGE (White) | RESPONSE (Gray)
Byte | Field Description | Byte | Field Description
0 | Frame (0xFE) | 0 | Frame (0xFE)
1, 2 | Length (0x0005) | 1, 2 | Length (0x0067)
3, 4 | Message Type (0x0007) | 3, 4 | Message Type (0x0007)
5 | Reserved (0x00) | 5 | Reserved (0x00)
6 | Sequence Number | 6 | Same Sequence Number
7 | Logical Node ID | 7 | Logical Node ID
8 | Checksum | 8, 9 | Status MSB, LSB
|  | 10 | Slot 0* Card Type
|  | 11 | Slot 1* Card Type (Response continued below.)
: | Card Type 0x00 8-Span ST1LC 0x0 1 4-Span ST1LC 0x03 MFDSP 0x0A SS7 0x0B SE1LC 4-Span 0x0C SE1LC 8-Span 0x0E SJ1LC 4-Span 0x13 ISDN PRI 0x14 DASS2 0x15 DSP-ONE 0x16 T-ONE 8-Span 0x17 E-ONE 8-Span 0x18 T-ONE 16-Span 0x19 E-ONE 16-Span 0x1D J-ONE 8-Span 0x1E J-ONE 16-Span 0x1F DS3 0x33 Subrate Controller 0x42 EXNET Connect PCI H.100 0x50 SS7 PQ 0x54 EXNET ONE 0x60 VDAC 0x61 VDAC VOIP Module 0x65 IP Network Interface Series 2 0x6B DSP Series 2 0x6D IP Network Interface Series 2 VoIP Module 0x71 SS7 Series 3 0x72 CSP Matrix I/O 0x73 CSP Matrix 2000 0x75 CSP Matrix 1000 0x76 ISDN Series 3 0x79 IP Signaling Series 3 0x80 Virtual 32 Span VDAC-ONE or IP Media Series 2 0x91 IP Network Interface Series 3 0x92 Multi-Function Media I/O Plus 0xCA Multi-Function Media I/O 0xCC DS3 Standby I/O 0xCF VDAC I/O 0xD2 Virtual T1 16-Span 0xD5 Virtual E1/J1 16-Span
| 0xD8 CCS I/O Series 3 0xDB J-ONE Redundant I/O 0xDC J-ONE Standby I/O 0xDD DS3 Redundant I/O 0xDF CCS I/O 0xE0 E-ONE 75 Ohm Redundant I/O 0xE1 T-ONE 100 Ohm Redundant I/O 0xE2 E-ONE 120 Ohm Redundant I/O 0xE3 E-ONE 75 Ohm Standby I/O 0xE4 T-ONE 100 Ohm Standby I/O 0xE5 E-ONE 120 Ohm Standby I/O 0xE8 SS7 Multi-Protocol I/O 0xF0 Power Supply 0xF5 EXNET Ring I/O 0xF6 Rear Fan Tray 0xF7 SS7 Redundant I/O 0xF8 Front Fan Tray 0xF9 ISDN Redundant I/O 0xFA Midplane 0xFE Dead Card All subsequent data fields are not applicable and all other bytes in the message should be ignored. 0xFF Empty Slot All subsequent data fields are not applicable.
73 | Slot 63 Card Type
74-105 | Slot 64-95 Card Type - Virtual Slot Configuration (See Virtual Slots below.)
106 | Checksum

*Slot Numbers

Front of Chassis
0x000x0F Line Card Slots 015
0x000x03 Line Card Slots 03
0x10 Front Fan Tray
0x11 Power2/ PSC 2
0x12 Power1/PSC 1
0x16 Fan Tray
0x20 CSP Matrix Series 3 Card 1
0x21 CSP Matrix Series 3 Card 2
Back of Chassis
0x13 Midplane
0x14 CSP Matrix Card I/O for CPU1
0x15 CSP 2000 Matrix I/O for CPU2
0x16 Rear Fan Tray
0x300x3F Redundant Line Card I/Os
0x300x33 Redundant Line Card I/Os
Virtual
0x40-0x5F Virtual Slots

A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
A group of data bits in a specific format, with a flag at each end to indicate the beginning and the end of the frame.
Most Significant Bit
Least Significant Bit
Range of channels provided by T1 or E1 transmission service. A physical span is a group of channels taking up a single physical wire. A logical span is a group of channels taking up less than a single logical wire, or carried over more than one physical wire.
See Signaling System Number Seven.
See Integrated Services Digital Network.
Digital Signal Processor
Excel's open architecture, proprietary, 1.3 Gbps fiber optic network using a packet-based protocol.
Peripheral Component Interconnect
Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).
Digital communications link - voice, data, and video at a 1.544 Mbps rate (24 64 Kbps channels)
A digital communications link - voice, data, and video at a 2.048 Mbps rate; 30B/2D or 31B/1D (ISDN); non-North American version of T1.
See Common Channel Signaling.