0x0647 Receive Modem Type

Use this TLV in the Generic Card Configure (0x0122) message to set the Receive Modem Type.

Byte | Description
0, 1 | Tag: 0x0647 Receive Modem Type
2, 3 | Length: 0x0002
4, 5 | Value[0-1]: Modems to advertise in the DIS 0x0001 V27 0x0002 V29 0x0008 V17 0x000B (V.29, V.27, V.17) default

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.