0x0616 DSP Series 2 Overload Statistics

This TLV is included in the response to the Statistics Query message (0x0121), in response to a DSP Overload Statistics query.

Byte | Description
0, 1 | Tag: 0x0616 DSP Series 2 Overload Statistics
2, 3 | Length: 0x001D
4 | Value[0]: DSP Series 2 Module
5 | Value[1]: DSP Chip
6-9 | Value[2-5]: VRA Process Delay Process Time of Cached Play Files, in microseconds
10-13 | Value[6-9]: Maximum VRA Process Delay Maximum Process Time of Cached Play Files, in microseconds.
14-17 | Value[10-13]: Average VRA Process Delay Average Process Time of Cached Play Files, in microseconds.
18-21 | Value[14-17]: VRA IO Queue Delay Process Time of Non-Cached Play and Record Files in microseconds.
22-25 | Value[18-21]: Maximum VRA IO Queue Delay Maximum Process Time of Non-Cached Play and Record Files, in microseconds.
26-29 | Value[22-25]: Average VRA IO Queue Delay Average Process Time of Non-Cached Play and Record Files, in microseconds.
30 | Value[26]: Percent CPU Idle
31 | Value[27]: Minimum Percent CPU Idle Time
32 | Value[28]: Average Percent CPU Idle Time

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Digital Signal Processor