0x05F6 DSP Series 2 Cache Statistics

This TLV is included in the response to the Statistics Query message. It reports cache accesses, hits, and misses, as well as average free blocks for a specific DSP chip. The history of these statistics is kept.

Byte | Description
0, 1 | Tag: 0x05F6 Cache Statistics
2, 3 | Length: 0x0010
4 | Value[0] Module Number 0x00 - DSP Module 0 0x01 - DSP Module 1 0xFF - Main board
5 | Value[1]: Processor Number Valid Range - 0-3 0x00 for main board processor
6-9 | Value[2-3]: Cache Accesses
10-13 | Value[6-9]: Cache Misses
14-17 | Value[10-13]: Cache Hits
18, 19 | Value[14, 15]: Average Free Blocks

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Digital Signal Processor