You are here: CSP Hardware Product Descriptions > 1 Chassis > Dialogic® CSP 2040 Chassis - CSN-CHA-1112/ CSN-CHA-1112R

Dialogic® CSP 2040 Chassis - CSN-CHA-1112/
CSN-CHA-1112R

Description

The Dialogic® CSP 2040, a compact chassis configuration of the Dialogic® Converged Services Platform (CSP) is designed to meet the demands of the telecommunication industry by delivering reliability, scalability and performance in a low-cost compact environment.

The CSP 2040 chassis accommodates up to 1,024 ports. The CSP 2040 is a compact chassis with seven front slots. The system is fully redundant and the cards are hot swappable. This chassis has one fan tray to ensure proper air flow and cooling. Blockout cards are required for proper air flow and cooling. Any unoccupied line card slot or I/O card slot should have a Blockout card installed.

The CSP 2040 can handle a maximum of 32 spans regardless of the line card type installed. It is compatible with the CSP 2090 hardware and software, allowing for easy expansion.

The CSP 2040 supports common channel signaling packet engines for both ISDN and SS7 communications. Line protocol cards include E1, T1 and J1 services. Standard and custom tone generation and reception, precise call analysis, conferencing and voice recorded announcements are provided through an advanced Digital Signal Processing unit available for the CSP.

Features

The CSP 2040 chassis consists of the following:

• One fan tray for cooling

• A midplane bus, which is a high-speed communication line for connecting individual line cards and I/O cards

• A seven card slot chassis (with dedicated CSP Matrix Series 3 cards slots and a Power card slot)

• Mounting brackets so the chassis can be mounted in a 19" or 23" rack.

Configuration Information

The part number, serial number, model number, and revision are located on the side of the chassis.

Specifications

The CSP 2040 chassis is designed to the following electrical, physical and environmental specifications.

Electrical | Specification
--- | ---
Input Power Requirement | -48 V DC, 10A (maximum)
Input Voltage Range | -40 V DC to -60 V DC

Physical | Specification
--- | ---
Height | 17.8 cm (7.0 in.)
Width | 43.5 cm (17.125 in.)
Depth | 48.2 cm (19.0 in.)
Weight | 18 kg (40 lb.) (loaded chassis)

Environmental | Specification
--- | ---
Temperature - Storage | -40~C to 70~C (-40~F to 158~F)
Temperature - Operation | 0~C to 50~C (32~F to 122~F)
Temperature Shock - Storage | -40~C to 70~C to -40~C (-40~F to 158~F to -40~F) @ 5~C/min.
Temperature Shock - Operation | 0~C to 50~C (32~F to 122~F) @ 10~C/min.
Humidity - Operating | 5% to 85%
Altitude | Up to 4000 m (13,123 ft.)

Front View

The front of the chassis has dedicated slots for two CSP Matrix Series 3 cards and one Power card. Slots 0-3 are for the other line cards.

Rear View

The rear of the chassis has dedicated slots for the CSP Matrix Series 3 I/O cards. Slots 0-3 are for the other I/O cards. The power input panel is also located at the rear of the chassis

Cross Sectional View

This shows the approximate location of the fan tray, midplane and front and rear card cages.

An Internet Protocol enhanced service node that supports the deployment of voice and data services in circuit, packet, and converged networks. The Converged Services Platform (CSP) features an open and multi-functional platform design that enables developers to quickly create and deliver new revenue-generating services for both legacy and next-generation networks.
See Integrated Services Digital Network.
See Signaling System Number Seven.
A digital communications link - voice, data, and video at a 2.048 Mbps rate; 30B/2D or 31B/1D (ISDN); non-North American version of T1.
Digital communications link - voice, data, and video at a 1.544 Mbps rate (24 64 Kbps channels)