0x01EB Initial Media Inactivity Timeout (IP Network Interface Series 2 Card)

Allows you to create a timer for monitoring the first incoming packet (for example, RTP, RTCP, or T.38) for each channel. If the timer expires before the first packet is received, a PPL Event Indication is generated, with an Event ID of 0x07.

Used in:
0x1E Generic PPL ICB in:
Resource Attribute Configure message
Route Control message
Outseize Control message

Byte | Description
0, 1 | Tag 0x01EB
2, 3 | Length 0x0004
4, 5 | Value[0, 1] 0x0000
6, 7 | RTP Timer Timeout Value (2 Bytes - 10 ms increments) 0x0000 - 0xFFFF ms 0x0000 is the default, and it means that the timer is disabled. Any other value automatically enables the timer to that value.

Real-Time Transport Protocol. Supports transport of real-time data like interactive voice and video over packet-switched networks.
Real-Time Transport Control Protocol.
See Programmable Protocol Language.
See Information Control Block.
Outgoing call setup during real-time call processing on a specific channel.