0x20 SS7 SCCP Parameters

Used in:
PPL Event Indication message
PPL Event Request message

ICB Type | 0x02 (Data)
ICB ID | 0x20
Data Length | Variable
Data[0] | Raw Parameter Data Parameter Length Data
Data[n] | :

See Programmable Protocol Language.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.
See Information Control Block.