MTP3 TLAC PPL Event Indications

Event ID | Event
--- | ---
0x0000 | Remote processor outage. A single ICB of type Q.752 Parameters is included with the following parameter: 0x0000 Timestamp 0x0001 Interval sequence number
0x0001 | Remote processor restored. A single ICB of type Q.752 Parameters is included with the following parameter: 0x0000 Timestamp 0x0001 Interval sequence number
0x0002 | Local inhibit. A single ICB of type Q.752 Parameters is included with the following parameter: 0x0000 Timestamp 0x0001 Interval sequence number
0x0003 | Local uninhibit. A single ICB of type Q.752 Parameters is included with the following parameter: 0x0000 Time stamp 0x0001 Interval sequence number
0x0004 | Remote inhibit. A single ICB of type Q.752 Parameters is included with the following parameter: 0x0000 Time stamp 0x0001 Interval sequence number
0x0005 | Remote uninhibit. A single ICB of type Q.752 Parameters is included with the following parameter: 0x0000 Time stamp 0x0001 Interval sequence number

See Information Control Block.