You are here: CSP API Reference > 1 EXS & SwitchKit API Messages > NGA Configure Query 0x0131

NGA Configure Query 0x0131

SwitchKit Name

NGAConfigureQuery

Type

EXS and SwitchKit API message

Description

NGA Configure Query 0x0131

Queries the M3UA objects for their service state.

Sent by

Host application

Related API Messages

NGA Configure (0x0130)
NGA Service Configure (0x0160)
NGA Service Query (0x0161)
NGA State Notify (0x0163)
NGA State Query (0x0162)

SwitchKit Code

C Structure

typedef struct {

UBYTE AddrInfo[30];

UBYTE DataType;

UBYTE TLVCount;

UBYTE Data[221];

} XL_NGAConfigureQuery;

C Structure Response

typedef struct {

unsigned short Status;

UBYTE reserved6[13];

UBYTE AddrInfo[30];

UBYTE DataType;

UBYTE TLVCount;

UBYTE Data[219];

} XL_NGAConfigureQueryAck;

C++ Class

class XLC_NGAConfigureQuery : public XLC_OutboundMessage {

public:

const UBYTE *getAddrInfo() const;

UBYTE *getAddrInfo();

void setAddrInfo(UBYTE *x);

void setAIBType(UBYTE x);

UBYTE getAIBType();

void setAECount(UBYTE x);

UBYTE getAECount();

void addAE(UBYTE AEpos, UBYTE AEtype, UBYTE AElen, UBYTE* AEvalue);

UBYTE* getAE(int AEpos);

void setAIBData(UBYTE* AIBDataPtr, UBYTE AIBDataLen);

UBYTE* getAIBData();

UBYTE getDataType() const;

void setDataType(UBYTE x);

UBYTE getTLVCount() const;

void setTLVCount(UBYTE x);

const UBYTE *getData() const;

UBYTE *getData();

void setData(UBYTE *x);

};

C++ Class Response

class XLC_NGAConfigureQueryAck : public

XLC_AcknowledgeMessage {

public:

unsigned short getStatus() const;

void setStatus(unsigned short x);

const UBYTE *getAddrInfo() const;

UBYTE *getAddrInfo();

void setAddrInfo(UBYTE *x);

void setAIBType(UBYTE x);

UBYTE getAIBType();

void setAECount(UBYTE x);

UBYTE getAECount();

void addAE(UBYTE AEpos, UBYTE AEtype, UBYTE AElen, UBYTE* AEvalue);

UBYTE* getAE(int AEpos);

void setAIBData(UBYTE* AIBDataPtr, UBYTE AIBDataLen);

UBYTE* getAIBData();

; UBYTE getDataType() const;

void setDataType(UBYTE x);

UBYTE getTLVCount() const;

void setTLVCount(UBYTE x);

const UBYTE *getData();

UBYTE *getData();

void setData(UBYTE *x);

};

EXS API Hex Format

MESSAGE (White) | RESPONSE (Gray)
Byte | Field Description | Byte | Field Description
0 | Frame (0xFE) | 0 | Frame (0xFE)
1, 2 | Length (0x00NN) | 1, 2 | Length (0x0007)
3, 4 | Message Type (0x0131) | 3, 4 | Message Type (0x0131)
5 | Reserved (0x00) | 5 | Reserved (0x00)
6 | Sequence Number | 6 | Same Sequence Number
7 | Logical Node ID | 7 | Logical Node ID
: | AIBs Address Method 0x03 - Item | 8 | Data Type 0x00 TLVs
9 | Number of TLVs to Follow
: | TLVs 0x904A Protocol Query 0x9050 General Query Data 0x904C Application Server Process Query 0x904E Signaling Gateway Process Query 0x904D Signaling Gateway Query 0x904F Connection Query 0x9051 Application Server State Query 0xE002 Service State
Number of AEs to Follow
AEs 0x67 Functional Area 0x08 SS7 Stack 0x64 Global Object Type 0xFFFF - Complete list of objects
: | Checksum | : | Checksum

A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
The condition of a component at a given instant. The current "context" of a PPL object, such as Idle, Seizing, Answered. In PPL files, a State is represented by a circle.
A group of data bits in a specific format, with a flag at each end to indicate the beginning and the end of the frame.