0x01C9 Primary Matrix IP Port

Use this TLV to specify the IP address and port number for the primary Call Agent. The port number must be greater than 0x0400 (1024).

Used in:
VoIP Protocol Query message
VoIP Protocol Configure message

Byte | Description
0, 1 | Tag 0x01C9
2, 3 | Length 0x0006
4-7 | Value[0-3] IP Address
8, 9 | Value[1, 2] Port Number

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).
A 32-bit address, used in IP routing, which includes a Network address identifier assigned by a central authority and a Host ID (an end station identifier assigned by a LAN administrator).
The point in the Excel platform where a DS0 connects to a network. Also known as a "socket."