0x0020 IP Signaling Series 3 Card Interface Status

Used in:
IP Signaling Series 3 Card Status Report message (0x0105)

Byte | Description
0, 1 | Tag 0x0020
2, 3 | Length 0x0004
4 | Value[0] DSM FSM State Values, MSB 0x00
5 | Value[1] DSM FSM State Values, LSB 0xFF FSM uninitialized 0x01 FSM initialized 0x02 FSM waiting for socket accessible indication 0x03 FSM waiting for socket inaccessible indication 0x04 FSM waiting for status request from the call server 0x05 FSM waiting for channel status request from the call server 0x06 FSM active 0x07 FSM inactive
6 | Value[2] Call Server Values, MSB 0x00
7 | Value[3] Call Server Values, LSB 0x01 Call server socket inaccessible 0x02 Call server socket accessible 0x03 Call server open failed 0x04 Call server close failed 0x05 Call server link down

Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
The condition of a component at a given instant. The current "context" of a PPL object, such as Idle, Seizing, Answered. In PPL files, a State is represented by a circle.
Most Significant Bit
Least Significant Bit