You are here: CSP API Reference > 1 EXS & SwitchKit API Messages > Start Dial Configure 0x0013

Start Dial Configure 0x0013

SwitchKit Name

StartDialConfig

Type

EXS API and SwitchKit API message

Description

Start Dial Configure 0x0013

This message allows the host to change the default start dial types.

Sent by

Host

SwitchKit Code

Configuration

StartDialConfig (

Node = integer,

Range = StartSpan:StartChan - EndSpan:EndChan,

StartDialType = integer,

StartDialValue = integer);

C Structure

typedef struct {

unsigned short StartSpan;

UBYTE StartChannel;

unsigned short EndSpan;

UBYTE EndChannel;

UBYTE StartDialType;

UBYTE StartDialValue;

} XL_StartDialConfig;

C++ Class

class XLC_StartDialConfig : public XLC_ChanRangeMessage {

public:

unsigned short getStartSpan() const;

void setStartSpan(unsigned short x);

UBYTE getStartChannel() const;

void setStartChannel(UBYTE x);

unsigned short getEndSpan() const;

void setEndSpan(unsigned short x);

UBYTE getEndChannel() const;

void setEndChannel(UBYTE x);

UBYTE getStartDialType() const;

void setStartDialType(UBYTE x);

UBYTE getStartDialValue() const;

void setStartDialValue(UBYTE x);

};

EXS API Hex Format

MESSAGE (White) | RESPONSE (Gray)
Byte | Field Description | Byte | Field Description
0 | Frame (0xFE) | 0 | Frame (0xFE)
1, 2 | Length (0x00NN) | 1, 2 | Length (0x0007)
3, 4 | Message Type (0x0013) | 3, 4 | Message Type (0x0013)
5 | Reserved (0x00) | 5 | Reserved (0x00)
6 | Sequence Number | 6 | Same Sequence Number
7 | Logical Node ID | 7 | Logical Node ID
8 : | AIB Address Method 0x01 - Range | 8, 9 | Status (MSB, LSB)
10 | Checksum
Number of AEs to follow |
AEs 0x0D Channel(Starting) 0x0D Channel (Ending)
: | Start Dial Type 0x01 Incoming Start Dial 0x02 Outgoing Start Dial
: | Start Dial Value The value of this field depends on the value of the Start Dial Type field. 0x01 Incoming Start Dial 0x01 Wink Start 0x02 Delay Dial 0x03 Immediate 0x04 Dial Tone 0x02 Outgoing Start Dial 0x01 Wink Start 0x02 Delay Dial 0x03 Fixed Pause 0x04 Dial Tone
: | Checksum

A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
A group of data bits in a specific format, with a flag at each end to indicate the beginning and the end of the frame.
See Address Information Block.
Most Significant Bit
Least Significant Bit
Momentary interruption in a single frequency tone indicating the distant switch is ready to receive the digits just dialed.