0x0141 Modify Connection

Use this TLV to change the connection type of an established connection between two channels without having to park the channels during the transition. Add this TLV to the Connect with Data message along with the Connection Type TLV (0x0612). If you do not include the Connection Type TLV, the Modified Connection defaults to a two-way connection.

Used in:
0x1E Generic PPL ICB in:
Connect with Data message

Byte | Description
0, 1 | Tag 0x0141 Modify Connection
2, 3 | Length 0x0002
4,5 | Value[0, 1] 0x0000 - Apply changes unconditionally (default)

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
See Programmable Protocol Language.
See Information Control Block.