0x0021 SS7 TCAP Parameters

Used in:
PPL Event Indication message
PPL Event Request message

ICB Type | 0x03 (Extended)
ICB ID | 0x0021
ICB Length (2 Bytes) | Variable
TCAP Dialogue ID (4 Bytes) |
Parameter Type (2 Bytes) |
Parameter Length (2 Bytes) |
Parameter Data |

See Programmable Protocol Language.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.
See Information Control Block.
See Transaction Capability Application Part.